You have to import the presets via the "**Preset Action**" menu

Press the Select encoder to open a pop-up menu in the display. Here, you can select the desired options and confirm by pressing on the **Select** encoder:

**Start Receive:** Puts Protein in a receive mode for multiple sound presets as MIDI SysEx dump from any external MIDI source. Here, you can set the slot from which onwards received presets will be stored. No existing presets will be overwritten but instead the next empty slot chosen. You must either confirm or cancel the final start of the process.

Du musst die Presets über das „**Preset Action Menu**“ importieren.

Drücke den "Select" Encoder, um ein Popup-Menü im Display zu öffnen.  Hier kannst du die gewünschten Optionen auswählen und durch Drücken des  "Select" Encoders bestätigen und „Start Receive“ auswählen:

**Start Receive:** Versetzt Protein in einen Empfangsmodus für  mehrere Sound-Presets als MIDI SysEx Dump von einer beliebigen externen  MIDI-Quelle. Hier kannst du den Speicherplatz festlegen, ab dem  empfangene Presets gespeichert werden sollen. Vorhandene Presets werden  nicht überschrieben, sondern es wird der nächste freie Speicherplatz  ausgewählt. Du musst den endgültigen Start des Vorgangs entweder  bestätigen oder abbrechen.